From e7a9cc3cc00b40e0bc2bae40bd2ece0e48fa51d5 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ar=C4=B1n=C3=A7=20=C3=9CNAL?= <arinc.unal@arinc9.com>
Date: Mon, 22 Apr 2024 10:15:22 +0300
Subject: [PATCH 15/15] net: dsa: mt7530: explain exposing MDIO bus of MT7531AE
 better
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Unlike MT7531BE, the GPIO 6-12 pins are not used for RGMII on MT7531AE.
Therefore, the GPIO 11-12 pins are set to function as MDC and MDIO to
expose the MDIO bus of the switch. Replace the comment with a better
explanation.

Signed-off-by: Arınç ÜNAL <arinc.unal@arinc9.com>
---
 drivers/net/dsa/mt7530.c | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -2639,7 +2639,10 @@ mt7531_setup(struct dsa_switch *ds)
 	if (!priv->p5_sgmii) {
 		mt7531_pll_setup(priv);
 	} else {
-		/* Let ds->slave_mii_bus be able to access external phy. */
+		/* Unlike MT7531BE, the GPIO 6-12 pins are not used for RGMII on
+		 * MT7531AE. Set the GPIO 11-12 pins to function as MDC and MDIO
+		 * to expose the MDIO bus of the switch.
+		 */
 		mt7530_rmw(priv, MT7531_GPIO_MODE1, MT7531_GPIO11_RG_RXD2_MASK,
 			   MT7531_EXT_P_MDC_11);
 		mt7530_rmw(priv, MT7531_GPIO_MODE1, MT7531_GPIO12_RG_RXD3_MASK,
