From ac7b46693a0d12f213eadf06884996bde9c478d3 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 6 Nov 2019 13:57:48 +0000
Subject: [PATCH 0184/1085] staging: vchiq_arm: Register vcsm-cma as a platform
 driver

Following the same pattern as bcm2835-camera and bcm2835-audio,
register the vcsm-cma driver as a platform driver

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
+++ b/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -67,6 +67,7 @@ struct vchiq_state g_state;
 
 static struct platform_device *bcm2835_camera;
 static struct platform_device *bcm2835_audio;
+static struct platform_device *vcsm_cma;
 
 struct vchiq_drvdata {
 	const unsigned int cache_line_size;
@@ -1824,6 +1825,7 @@ static int vchiq_probe(struct platform_d
 		goto error_exit;
 	}
 
+	vcsm_cma = vchiq_register_child(pdev, "vcsm-cma");
 	bcm2835_camera = vchiq_register_child(pdev, "bcm2835-camera");
 	bcm2835_audio = vchiq_register_child(pdev, "bcm2835_audio");
 
@@ -1839,6 +1841,7 @@ static void vchiq_remove(struct platform
 {
 	platform_device_unregister(bcm2835_audio);
 	platform_device_unregister(bcm2835_camera);
+	platform_device_unregister(vcsm_cma);
 	vchiq_debugfs_deinit();
 	vchiq_deregister_chrdev();
 }
