From 9b6bfad9070a95d19973be17177e5d9220cbbf1f Mon Sep 17 00:00:00 2001
From: Rick Wertenbroek <rick.wertenbroek@gmail.com>
Date: Thu, 7 Mar 2024 10:53:18 +0100
Subject: [PATCH] phy: rockchip: Fix typo in function names

Several functions had "rochchip" instead of "rockchip" in their name.
Replace "rochchip" by "rockchip".

Signed-off-By: Rick Wertenbroek <rick.wertenbroek@gmail.com>
Reviewed-by: Heiko Stuebner <heiko@sntech.de>
Link: https://lore.kernel.org/r/20240307095318.3651498-1-rick.wertenbroek@gmail.com
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/phy/rockchip/phy-rockchip-naneng-combphy.c |  4 ++--
 drivers/phy/rockchip/phy-rockchip-snps-pcie3.c     | 12 ++++++------
 2 files changed, 8 insertions(+), 8 deletions(-)

--- a/drivers/phy/rockchip/phy-rockchip-naneng-combphy.c
+++ b/drivers/phy/rockchip/phy-rockchip-naneng-combphy.c
@@ -248,7 +248,7 @@ static int rockchip_combphy_exit(struct
 	return 0;
 }
 
-static const struct phy_ops rochchip_combphy_ops = {
+static const struct phy_ops rockchip_combphy_ops = {
 	.init = rockchip_combphy_init,
 	.exit = rockchip_combphy_exit,
 	.owner = THIS_MODULE,
@@ -367,7 +367,7 @@ static int rockchip_combphy_probe(struct
 		return ret;
 	}
 
-	priv->phy = devm_phy_create(dev, NULL, &rochchip_combphy_ops);
+	priv->phy = devm_phy_create(dev, NULL, &rockchip_combphy_ops);
 	if (IS_ERR(priv->phy)) {
 		dev_err(dev, "failed to create combphy\n");
 		return PTR_ERR(priv->phy);
--- a/drivers/phy/rockchip/phy-rockchip-snps-pcie3.c
+++ b/drivers/phy/rockchip/phy-rockchip-snps-pcie3.c
@@ -182,7 +182,7 @@ static const struct rockchip_p3phy_ops r
 	.phy_init = rockchip_p3phy_rk3588_init,
 };
 
-static int rochchip_p3phy_init(struct phy *phy)
+static int rockchip_p3phy_init(struct phy *phy)
 {
 	struct rockchip_p3phy_priv *priv = phy_get_drvdata(phy);
 	int ret;
@@ -205,7 +205,7 @@ static int rochchip_p3phy_init(struct ph
 	return ret;
 }
 
-static int rochchip_p3phy_exit(struct phy *phy)
+static int rockchip_p3phy_exit(struct phy *phy)
 {
 	struct rockchip_p3phy_priv *priv = phy_get_drvdata(phy);
 
@@ -214,9 +214,9 @@ static int rochchip_p3phy_exit(struct ph
 	return 0;
 }
 
-static const struct phy_ops rochchip_p3phy_ops = {
-	.init = rochchip_p3phy_init,
-	.exit = rochchip_p3phy_exit,
+static const struct phy_ops rockchip_p3phy_ops = {
+	.init = rockchip_p3phy_init,
+	.exit = rockchip_p3phy_exit,
 	.set_mode = rockchip_p3phy_set_mode,
 	.owner = THIS_MODULE,
 };
@@ -275,7 +275,7 @@ static int rockchip_p3phy_probe(struct p
 		return priv->num_lanes;
 	}
 
-	priv->phy = devm_phy_create(dev, NULL, &rochchip_p3phy_ops);
+	priv->phy = devm_phy_create(dev, NULL, &rockchip_p3phy_ops);
 	if (IS_ERR(priv->phy)) {
 		dev_err(dev, "failed to create combphy\n");
 		return PTR_ERR(priv->phy);
