From 24559788384916041a0bbf54c32e2a16b612d247 Mon Sep 17 00:00:00 2001
From: John Clark <inindev@gmail.com>
Date: Mon, 25 Dec 2023 22:32:16 +0000
Subject: [PATCH] arm64: dts: rockchip: correct gpio_pwrctrl1 typo on nanopc-t6

Both rk806_dvs1_null and rk806_dvs2_null duplicate gpio_pwrctrl2 and
gpio_pwrctrl1 is not set. This patch sets gpio_pwrctrl1.

Signed-off-by: John Clark <inindev@gmail.com>
Link: https://lore.kernel.org/r/20231225223226.17690-1-inindev@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
@@ -590,7 +590,7 @@
 		#gpio-cells = <2>;
 
 		rk806_dvs1_null: dvs1-null-pins {
-			pins = "gpio_pwrctrl2";
+			pins = "gpio_pwrctrl1";
 			function = "pin_fun0";
 		};
 
