#
# Copyright (c) 2015 The Linux Foundation. All rights reserved.
# Copyright (c) 2011-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

ipq806x_setup_interfaces()
{
	local board="$1"

	case "$board" in
	arris,tr4400-v2)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth2"
		;;
	askey,rt4230w-rev6 |\
	asrock,g10 |\
	nec,wg2600hp |\
	buffalo,wxr-2533dhp |\
	compex,wpq864 |\
	netgear,d7800 |\
	netgear,r7500 |\
	netgear,r7500v2 |\
	qcom,ipq8064-ap148 |\
	linksys,e8350-v1 |\
	linksys,ea7500-v1 |\
	linksys,ea8500 |\
	nec,wg2600hp3 |\
	netgear,r7800 |\
	netgear,xr500 |\
	netgear,xr450 |\
	tplink,c2600 |\
	tplink,vr2600v |\
	tplink,ad7200 |\
	zyxel,nbg6817)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "wan"
		ucidef_set_network_device_conduit "lan1" "eth1"
		ucidef_set_network_device_conduit "lan2" "eth1"
		ucidef_set_network_device_conduit "lan3" "eth1"
		ucidef_set_network_device_conduit "lan4" "eth1"
		ucidef_set_network_device_conduit "wan" "eth0"
		;;
	asus,onhub |\
	ruijie,rg-mtfi-m520 |\
	tplink,onhub)
		ucidef_set_interfaces_lan_wan "lan1" "wan"
		ucidef_set_network_device_conduit "lan1" "eth1"
		ucidef_set_network_device_conduit "wan" "eth0"
		;;
	edgecore,ecw5410 |\
	extreme,ap3935)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;
	qcom,ipq8064-ap161)
		ucidef_set_interface_lan "eth1 eth2 lan1 lan2 lan3 lan4" "wan"
		;;
	qcom,ipq8064-db149)
		ucidef_set_interface_lan "eth1 eth2 eth3 lan1 lan2 lan3 lan4" "wan"
		;;
	fortinet,fap-421e |\
	ubnt,unifi-ac-hd)
		ucidef_set_interface_lan "eth0 eth1"
		;;
	xiaomi,mi-router-hd)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3" "wan"
		ucidef_set_network_device_conduit "lan1" "eth1"
		ucidef_set_network_device_conduit "lan2" "eth1"
		ucidef_set_network_device_conduit "lan3" "eth1"
		ucidef_set_network_device_conduit "wan" "eth0"
		;;
	meraki,mr42)
		ucidef_set_interface_lan "eth0"
		;;
	meraki,mr52)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		;;
	*)
		echo "Unsupported hardware. Network interfaces not intialized"
		;;
	esac
}

ipq806x_setup_macs()
{
	local board="$1"

	case "$board" in
		linksys,ea7500-v1)
			hw_mac_addr=$(mtd_get_mac_ascii devinfo hw_mac_addr)
			ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
			ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 1)"
		;;
		linksys,ea8500)
			hw_mac_addr=$(mtd_get_mac_ascii devinfo hw_mac_addr)
			ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
			ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 1)"
		;;
		linksys,e8350-v1 |\
		zyxel,nbg6817)
			hw_mac_addr=$(mtd_get_mac_ascii 0:appsblenv ethaddr)
			ucidef_set_interface_macaddr "lan" "$(macaddr_add $hw_mac_addr 2)"
			ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 3)"
		;;
		ruijie,rg-mtfi-m520)
			hw_mac_addr=$(mtd_get_mac_ascii PRODUCTINFO ethaddr)
			ucidef_set_interface_macaddr "wan" "$hw_mac_addr"
			ucidef_set_interface_macaddr "lan" "$(macaddr_add $hw_mac_addr 1)"
		;;
		asrock,g10)
			hw_mac_addr=$(mtd_get_mac_ascii hwconfig HW.LAN.MAC.Address)
			ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
			hw_mac_addr=$(mtd_get_mac_ascii hwconfig HW.WAN.MAC.Address)
			ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 1)"
		;;
	esac
}

board_config_update
board=$(board_name)

ipq806x_setup_macs $board
ipq806x_setup_interfaces $board

board_config_flush

exit 0
