<!---======================= begin_copyright_notice ============================

Copyright (C) 2020-2021 Intel Corporation

SPDX-License-Identifier: MIT

============================= end_copyright_notice ==========================-->

 

## Opcode

  DIV = 0x03

## Format

| | | | | |
| --- | --- | --- | --- | --- |
| 0x03(DIV) | Exec_size | Pred | Dst | Src0 | Src1 |


## Semantics




                    for (i = 0; < exec_size; ++i) {
                      if (ChEn[i]) {
                        dst[i] = src0[i] / src1[i];
                      }
                    }

## Description



    Divides <src0> by <src1> component-wise, and stores the result into <dst>.

- **Exec_size(ub):** Execution size
 
  - Bit[2..0]: size of the region for source and destination operands
 
    - 0b000:  1 element (scalar) 
    - 0b001:  2 elements 
    - 0b010:  4 elements 
    - 0b011:  8 elements 
    - 0b100:  16 elements 
    - 0b101:  32 elements 
  - Bit[7..4]: execution mask (explicit control over the enabled channels)
 
    - 0b0000:  M1 
    - 0b0001:  M2 
    - 0b0010:  M3 
    - 0b0011:  M4 
    - 0b0100:  M5 
    - 0b0101:  M6 
    - 0b0110:  M7 
    - 0b0111:  M8 
    - 0b1000:  M1_NM 
    - 0b1001:  M2_NM 
    - 0b1010:  M3_NM 
    - 0b1011:  M4_NM 
    - 0b1100:  M5_NM 
    - 0b1101:  M6_NM 
    - 0b1110:  M7_NM 
    - 0b1111:  M8_NM
- **Pred(uw):** Predication control

- **Dst(vec_operand):** The destination operand. Operand class: general,indirect

- **Src0(vec_operand):** The first source operand. Operand class: general,indirect,immediate

- **Src1(vec_operand):** The second source operand. Operand class: general,indirect,immediate

#### Properties
- **Supported Types:** B,D,F,HF,UB,UD,UW,W 
- **Saturation:** Only when type is float 
- **Source Modifier:** arithmetic 


## Text
```
    

		[(<P>)] DIV[.sat]  (<exec_size>) <dst> <src0> <src1>
```



## Notes



		


Integer divide with signed inputs follow the rules below for the signs of the quotient and remainder.

  +------------+------------------+-----+-----+-----+-----+
  | Inputs:    |   Numerator      | \+  | \+  | \-  | \-  |
  +------------+------------------+-----+-----+-----+-----+
  |            |   Denominator    | \+  | \-  | \+  | \-  |
  +------------+------------------+-----+-----+-----+-----+
  | Outputs:   |   Quotient       | \+  | \-  | \-  | \+  |
  +------------+------------------+-----+-----+-----+-----+
  |            |   Remainder      | \+  | \+  | \-  | \-  |
  +------------+------------------+-----+-----+-----+-----+

Floating point divide (x/y) is implemented as x * INV(y).  DIVM provides the IEEE-conforming correctly rounded results.
