diff -urN linux-2.6.16.7/drivers/char/watchdog/Kconfig linux-2.6.16.7.new/drivers/char/watchdog/Kconfig
--- linux-2.6.16.7/drivers/char/watchdog/Kconfig	2006-04-17 23:53:25.000000000 +0200
+++ linux-2.6.16.7.new/drivers/char/watchdog/Kconfig	2006-04-22 23:23:53.000000000 +0200
@@ -460,6 +460,14 @@
 	  timer expired and no process has written to /dev/watchdog during
 	  that time.
 
+config MTX1_WATCHDOG
+	tristate "MTX-1 Hardware Watchdog"
+	depends on WATCHDOG && MIPS_MTX1
+	help
+	  Hardware driver for the AccessCube MTX-1 watchdog. This is a
+	  watchdog timer that will reboot the machine after a 100 seconds
+	  timer expired.
+
 # S390 Architecture
 
 config ZVM_WATCHDOG
diff -urN linux-2.6.16.7/drivers/char/watchdog/Makefile linux-2.6.16.7.new/drivers/char/watchdog/Makefile
--- linux-2.6.16.7/drivers/char/watchdog/Makefile	2006-04-17 23:53:25.000000000 +0200
+++ linux-2.6.16.7.new/drivers/char/watchdog/Makefile	2006-04-22 23:21:18.000000000 +0200
@@ -65,6 +65,7 @@
 
 # MIPS Architecture
 obj-$(CONFIG_INDYDOG) += indydog.o
+obj-$(CONFIG_MTX1_WATCHDOG) += mtx-1_watchdog.o
 
 # S390 Architecture
