diff -Nur linux-2.6.17/arch/mips/Kconfig linux-2.6.17-owrt/arch/mips/Kconfig
--- linux-2.6.17/arch/mips/Kconfig	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/arch/mips/Kconfig	2006-06-18 12:44:28.000000000 +0200
@@ -227,6 +227,17 @@
 	  either a NEC Vr5432 or QED RM5231. Say Y here if you wish to build
 	  a kernel for this platform.
 
+config MACH_ARUBA
+	bool "Support for the ARUBA product line"
+	select DMA_NONCOHERENT
+	select CPU_HAS_PREFETCH
+	select HW_HAS_PCI
+	select SWAP_IO_SPACE
+	select SYS_SUPPORTS_32BIT_KERNEL
+	select SYS_HAS_CPU_MIPS32_R1
+	select SYS_SUPPORTS_BIG_ENDIAN
+
+
 config MACH_JAZZ
 	bool "Jazz family of machines"
 	select ARC
diff -Nur linux-2.6.17/arch/mips/Makefile linux-2.6.17-owrt/arch/mips/Makefile
--- linux-2.6.17/arch/mips/Makefile	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/arch/mips/Makefile	2006-06-18 12:44:28.000000000 +0200
@@ -145,6 +145,14 @@
 #
 
 #
+# Aruba
+#
+
+core-$(CONFIG_MACH_ARUBA)	+= arch/mips/aruba/
+cflags-$(CONFIG_MACH_ARUBA)	+= -Iinclude/asm-mips/aruba
+load-$(CONFIG_MACH_ARUBA)	+= 0x80100000
+
+#
 # Acer PICA 61, Mips Magnum 4000 and Olivetti M700.
 #
 core-$(CONFIG_MACH_JAZZ)	+= arch/mips/jazz/
diff -Nur linux-2.6.17/drivers/net/Kconfig linux-2.6.17-owrt/drivers/net/Kconfig
--- linux-2.6.17/drivers/net/Kconfig	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/drivers/net/Kconfig	2006-06-18 12:44:28.000000000 +0200
@@ -187,6 +187,13 @@
 
 source "drivers/net/arm/Kconfig"
 
+config IDT_RC32434_ETH
+        tristate "IDT RC32434 Local Ethernet support"
+        depends on NET_ETHERNET
+        help
+        IDT RC32434 has one local ethernet port. Say Y here to enable it.
+        To compile this driver as a module, choose M here.
+
 config MACE
 	tristate "MACE (Power Mac ethernet) support"
 	depends on NET_ETHERNET && PPC_PMAC && PPC32
diff -Nur linux-2.6.17/drivers/net/Makefile linux-2.6.17-owrt/drivers/net/Makefile
--- linux-2.6.17/drivers/net/Makefile	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/drivers/net/Makefile	2006-06-18 12:44:28.000000000 +0200
@@ -38,6 +38,7 @@
 
 obj-$(CONFIG_OAKNET) += oaknet.o 8390.o
 
+obj-$(CONFIG_IDT_RC32434_ETH) += rc32434_eth.o
 obj-$(CONFIG_DGRS) += dgrs.o
 obj-$(CONFIG_VORTEX) += 3c59x.o
 obj-$(CONFIG_TYPHOON) += typhoon.o
diff -Nur linux-2.6.17/drivers/net/natsemi.c linux-2.6.17-owrt/drivers/net/natsemi.c
--- linux-2.6.17/drivers/net/natsemi.c	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/drivers/net/natsemi.c	2006-06-18 12:44:28.000000000 +0200
@@ -771,6 +771,49 @@
 static int netdev_get_eeprom(struct net_device *dev, u8 *buf);
 static struct ethtool_ops ethtool_ops;
 
+#ifdef CONFIG_MACH_ARUBA
+
+#include <linux/ctype.h>
+
+#ifndef ERR
+#define ERR(fmt, args...) printk("%s: " fmt, __func__, ##args)
+#endif
+
+static int parse_mac_addr(struct net_device *dev, char* macstr)
+{
+        int i, j;
+        unsigned char result, value;
+
+        for (i=0; i<6; i++) {
+                result = 0;
+                if (i != 5 && *(macstr+2) != ':') {
+                        ERR("invalid mac address format: %d %c\n",
+                            i, *(macstr+2));
+                        return -EINVAL;
+                }
+                for (j=0; j<2; j++) {
+                        if (isxdigit(*macstr) && (value = isdigit(*macstr) ? *macstr-'0' :
+                                                  toupper(*macstr)-'A'+10) < 16) {
+                                result = result*16 + value;
+                                macstr++;
+                        }
+                        else {
+                                ERR("invalid mac address "
+                                    "character: %c\n", *macstr);
+                                return -EINVAL;
+                        }
+                }
+
+                macstr++;
+                dev->dev_addr[i] = result;
+        }
+
+	dev->dev_addr[5]++;
+        return 0;
+}
+
+#endif
+
 static inline void __iomem *ns_ioaddr(struct net_device *dev)
 {
 	return (void __iomem *) dev->base_addr;
@@ -871,6 +914,7 @@
 		goto err_ioremap;
 	}
 
+#ifndef CONFIG_MACH_ARUBA
 	/* Work around the dropped serial bit. */
 	prev_eedata = eeprom_read(ioaddr, 6);
 	for (i = 0; i < 3; i++) {
@@ -879,6 +923,19 @@
 		dev->dev_addr[i*2+1] = eedata >> 7;
 		prev_eedata = eedata;
 	}
+#else
+	{
+		char mac[32];
+		unsigned char def_mac[6] = {00, 0x0b, 0x86, 0xba, 0xdb, 0xad};
+		extern char *getenv(char *e);
+		memset(mac, 0, 32);
+		memcpy(mac, getenv("ethaddr"), 17);
+		if (parse_mac_addr(dev, mac)){
+			printk("%s: MAC address not found\n", __func__);
+			memcpy(dev->dev_addr, def_mac, 6);
+		}
+	}
+#endif
 
 	dev->base_addr = (unsigned long __force) ioaddr;
 	dev->irq = irq;
diff -Nur linux-2.6.17/include/asm-mips/bootinfo.h linux-2.6.17-owrt/include/asm-mips/bootinfo.h
--- linux-2.6.17/include/asm-mips/bootinfo.h	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/include/asm-mips/bootinfo.h	2006-06-18 12:44:28.000000000 +0200
@@ -218,6 +218,17 @@
 #define MACH_GROUP_TITAN       22	/* PMC-Sierra Titan		*/
 #define  MACH_TITAN_YOSEMITE	1	/* PMC-Sierra Yosemite		*/
 
+
+/*
+ * Valid machtype for group ARUBA
+ */
+#define MACH_GROUP_ARUBA	23
+#define  MACH_ARUBA_UNKNOWN	0
+#define  MACH_ARUBA_AP60	1
+#define  MACH_ARUBA_AP65	2
+#define  MACH_ARUBA_AP70	3
+#define  MACH_ARUBA_AP40	4
+
 #define CL_SIZE			COMMAND_LINE_SIZE
 
 const char *get_system_type(void);
diff -Nur linux-2.6.17/include/asm-mips/cpu.h linux-2.6.17-owrt/include/asm-mips/cpu.h
--- linux-2.6.17/include/asm-mips/cpu.h	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/include/asm-mips/cpu.h	2006-06-18 12:45:56.000000000 +0200
@@ -54,6 +54,9 @@
 #define PRID_IMP_R14000		0x0f00
 #define PRID_IMP_R8000		0x1000
 #define PRID_IMP_PR4450		0x1200
+#define PRID_IMP_RC32334	0x1800
+#define PRID_IMP_RC32355	0x1900
+#define PRID_IMP_RC32365	0x1900
 #define PRID_IMP_R4600		0x2000
 #define PRID_IMP_R4700		0x2100
 #define PRID_IMP_TX39		0x2200
@@ -200,7 +203,8 @@
 #define CPU_SB1A		62
 #define CPU_74K			63
 #define CPU_R14000		64
-#define CPU_LAST		64
+#define CPU_RC32300		65
+#define CPU_LAST		65
 
 /*
  * ISA Level encodings
diff -Nur linux-2.6.17/include/asm-mips/mach-generic/irq.h linux-2.6.17-owrt/include/asm-mips/mach-generic/irq.h
--- linux-2.6.17/include/asm-mips/mach-generic/irq.h	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/include/asm-mips/mach-generic/irq.h	2006-06-18 12:44:28.000000000 +0200
@@ -8,6 +8,6 @@
 #ifndef __ASM_MACH_GENERIC_IRQ_H
 #define __ASM_MACH_GENERIC_IRQ_H
 
-#define NR_IRQS	128
+#define NR_IRQS	256
 
 #endif /* __ASM_MACH_GENERIC_IRQ_H */
diff -Nur linux-2.6.17/include/linux/kernel.h linux-2.6.17-owrt/include/linux/kernel.h
--- linux-2.6.17/include/linux/kernel.h	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17-owrt/include/linux/kernel.h	2006-06-18 12:44:28.000000000 +0200
@@ -329,6 +329,7 @@
 };
 
 /* Force a compilation error if condition is true */
+extern void BUILD_BUG(void);
 #define BUILD_BUG_ON(condition) ((void)sizeof(char[1 - 2*!!(condition)]))
 
 /* Trap pasters of __FUNCTION__ at compile-time */
