From c0612164b379ebc8964da6bc6f6ced9736dce488 Mon Sep 17 00:00:00 2001
From: Mathew McBride <matt@traverse.com.au>
Date: Tue, 17 Apr 2018 10:01:03 +1000
Subject: [PATCH] add DTS for Traverse LS1043 Boards

Signed-off-by: Mathew McBride <matt@traverse.com.au>
---
 arch/arm64/boot/dts/freescale/Makefile |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm64/boot/dts/freescale/traverse-ls1043v.dts

--- a/arch/arm64/boot/dts/freescale/Makefile
+++ b/arch/arm64/boot/dts/freescale/Makefile
@@ -21,7 +21,10 @@ dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-simu.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2088a-qds.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2088a-rdb.dtb
- 
+
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += traverse-ls1043v.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += traverse-ls1043s.dtb
+
 always		:= $(dtb-y)
 subdir-y	:= $(dts-dirs)
 clean-files	:= *.dtb
--- a/arch/arm64/boot/dts/freescale/traverse-ls1043s.dts
+++ b/arch/arm64/boot/dts/freescale/traverse-ls1043s.dts
@@ -330,3 +330,32 @@
 &sata {
 	status = "disabled";
 };
+
+/* Additions for Layerscape SDK (4.4/4.9) Kernel only
+ * These kernels need additional setup for FMan/QMan DMA shared memory
+ */
+
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
--- a/arch/arm64/boot/dts/freescale/traverse-ls1043v.dts
+++ b/arch/arm64/boot/dts/freescale/traverse-ls1043v.dts
@@ -251,3 +251,32 @@
 &sata {
 	status = "disabled";
 };
+
+/* Additions for Layerscape SDK (4.4/4.9) Kernel only
+ * These kernels need additional setup for FMan/QMan DMA shared memory
+ */
+
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
