diff --git a/drivers/mtd/nand/spi/Makefile b/drivers/mtd/nand/spi/Makefile
index 9c64d9fc..5f99ea72 100644
--- a/drivers/mtd/nand/spi/Makefile
+++ b/drivers/mtd/nand/spi/Makefile
@@ -1,3 +1,3 @@
 # SPDX-License-Identifier: GPL-2.0
-spinand-objs := core.o esmt.o gigadevice.o macronix.o micron.o paragon.o toshiba.o winbond.o xtx.o
+spinand-objs := core.o esmt.o etron.o gigadevice.o macronix.o micron.o paragon.o toshiba.o winbond.o xtx.o
 obj-$(CONFIG_MTD_SPI_NAND) += spinand.o
diff --git a/drivers/mtd/nand/spi/core.c b/drivers/mtd/nand/spi/core.c
index 9839ee44..9ab44217 100644
--- a/drivers/mtd/nand/spi/core.c
+++ b/drivers/mtd/nand/spi/core.c
@@ -898,6 +898,7 @@ static const struct nand_ops spinand_ops = {
 static const struct spinand_manufacturer *spinand_manufacturers[] = {
	&esmt_c8_spinand_manufacturer,
	&gigadevice_spinand_manufacturer,
+	&etron_spinand_manufacturer,
	&macronix_spinand_manufacturer,
	&micron_spinand_manufacturer,
	&paragon_spinand_manufacturer,
diff --git a/drivers/mtd/nand/spi/etron.c b/drivers/mtd/nand/spi/etron.c
new file mode 100644
index 00000000..653092be
--- /dev/null
+++ b/drivers/mtd/nand/spi/etron.c
@@ -0,0 +1,98 @@
+// SPDX-License-Identifier: GPL-2.0
+
+#include <linux/device.h>
+#include <linux/kernel.h>
+#include <linux/mtd/spinand.h>
+
+#define SPINAND_MFR_ETRON			0xd5
+
+
+static SPINAND_OP_VARIANTS(read_cache_variants,
+		SPINAND_PAGE_READ_FROM_CACHE_QUADIO_OP(0, 1, NULL, 0),
+		SPINAND_PAGE_READ_FROM_CACHE_X4_OP(0, 1, NULL, 0),
+		SPINAND_PAGE_READ_FROM_CACHE_DUALIO_OP(0, 1, NULL, 0),
+		SPINAND_PAGE_READ_FROM_CACHE_X2_OP(0, 1, NULL, 0),
+		SPINAND_PAGE_READ_FROM_CACHE_OP(true, 0, 1, NULL, 0),
+		SPINAND_PAGE_READ_FROM_CACHE_OP(false, 0, 1, NULL, 0));
+
+static SPINAND_OP_VARIANTS(write_cache_variants,
+		SPINAND_PROG_LOAD_X4(true, 0, NULL, 0),
+		SPINAND_PROG_LOAD(true, 0, NULL, 0));
+
+static SPINAND_OP_VARIANTS(update_cache_variants,
+		SPINAND_PROG_LOAD_X4(false, 0, NULL, 0),
+		SPINAND_PROG_LOAD(false, 0, NULL, 0));
+
+static int etron_ooblayout_ecc(struct mtd_info *mtd, int section,
+					struct mtd_oob_region *oobregion)
+{
+	if (section)
+		return -ERANGE;
+
+	oobregion->offset = 72;
+	oobregion->length = 56;
+
+	return 0;
+}
+
+static int etron_ooblayout_free(struct mtd_info *mtd, int section,
+			   struct mtd_oob_region *oobregion)
+{
+	if (section)
+		return -ERANGE;
+
+	oobregion->offset = 1;
+	oobregion->length = 71;
+
+	return 0;
+}
+
+static int etron_ecc_get_status(struct spinand_device *spinand, u8 status)
+{
+	switch (status & STATUS_ECC_MASK) {
+	case STATUS_ECC_NO_BITFLIPS:
+		return 0;
+
+	case STATUS_ECC_HAS_BITFLIPS:
+		/* Between 1-7 bitflips were corrected */
+		return 7;
+
+	case STATUS_ECC_MASK:
+		/* Maximum bitflips were corrected */
+		return 8;
+
+	case STATUS_ECC_UNCOR_ERROR:
+		return -EBADMSG;
+	}
+
+	return -EINVAL;
+}
+
+static const struct mtd_ooblayout_ops etron_ooblayout = {
+	.ecc = etron_ooblayout_ecc,
+	.free = etron_ooblayout_free,
+};
+
+static const struct spinand_info etron_spinand_table[] = {
+	SPINAND_INFO("EM73D044VCx",
+		     SPINAND_ID(SPINAND_READID_METHOD_OPCODE_ADDR, 0x1f),
+		     // bpc, pagesize, oobsize, pagesperblock, bperlun, maxbadplun, ppl, lpt, #t
+		     NAND_MEMORG(1, 2048, 128, 64, 2048, 40, 1, 1, 1),
+		     NAND_ECCREQ(8, 512),
+		     SPINAND_INFO_OP_VARIANTS(&read_cache_variants,
+					      &write_cache_variants,
+					      &update_cache_variants),
+		     SPINAND_HAS_QE_BIT,
+		     SPINAND_ECCINFO(&etron_ooblayout, etron_ecc_get_status)),
+};
+
+static const struct spinand_manufacturer_ops etron_spinand_manuf_ops = {
+};
+
+const struct spinand_manufacturer etron_spinand_manufacturer = {
+	.id = SPINAND_MFR_ETRON,
+	.name = "Etron",
+	.chips = etron_spinand_table,
+	.nchips = ARRAY_SIZE(etron_spinand_table),
+	.ops = &etron_spinand_manuf_ops,
+};
diff --git a/include/linux/mtd/spinand.h b/include/linux/mtd/spinand.h
index 2066962d..11d38d2f 100644
--- a/include/linux/mtd/spinand.h
+++ b/include/linux/mtd/spinand.h
@@ -261,6 +261,7 @@ struct spinand_manufacturer {

 /* SPI NAND manufacturers */
 extern const struct spinand_manufacturer esmt_c8_spinand_manufacturer;
+extern const struct spinand_manufacturer etron_spinand_manufacturer;
 extern const struct spinand_manufacturer gigadevice_spinand_manufacturer;
 extern const struct spinand_manufacturer macronix_spinand_manufacturer;
 extern const struct spinand_manufacturer micron_spinand_manufacturer;
