From 4823778b116c08e9c55dbc5b5042223289ea6a0c Mon Sep 17 00:00:00 2001
From: Frank Wunderlich <frank-w@public-files.de>
Date: Wed, 31 Mar 2021 15:34:37 +0200
Subject: [PATCH] net: mediatek: add flow offload for mt7623

mt7623 uses offload version 2 too

tested on Bananapi-R2

Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -3637,6 +3637,7 @@ static const struct mtk_soc_data mt2701_
 	.hw_features = MTK_HW_FEATURES,
 	.required_clks = MT7623_CLKS_BITMAP,
 	.required_pctl = true,
+	.offload_version = 2,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
 		.rxd_size = sizeof(struct mtk_rx_dma),
