From ffbeb183bf0e9e12fd607c5352f48420c32f588f Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Sat, 12 May 2012 23:04:17 +0200
Subject: [PATCH 61/79] MIPS: BCM63XX: export PSI size from nvram

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 arch/mips/bcm63xx/nvram.c                          |   11 +++++++++++
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_nvram.h |    2 ++
 2 files changed, 13 insertions(+)

--- a/arch/mips/bcm63xx/nvram.c
+++ b/arch/mips/bcm63xx/nvram.c
@@ -14,6 +14,8 @@
 
 #include <bcm63xx_nvram.h>
 
+#define BCM63XX_DEFAULT_PSI_SIZE	64
+
 static struct bcm963xx_nvram nvram;
 static int mac_addr_used;
 
@@ -82,3 +84,12 @@ int bcm63xx_nvram_get_mac_address(u8 *ma
 	return 0;
 }
 EXPORT_SYMBOL(bcm63xx_nvram_get_mac_address);
+
+int bcm63xx_nvram_get_psi_size(void)
+{
+	if (nvram.psi_size > 0)
+		return nvram.psi_size;
+
+	return BCM63XX_DEFAULT_PSI_SIZE;
+}
+EXPORT_SYMBOL(bcm63xx_nvram_get_psi_size);
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_nvram.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_nvram.h
@@ -31,4 +31,6 @@ u8 *bcm63xx_nvram_get_name(void);
  */
 int bcm63xx_nvram_get_mac_address(u8 *mac);
 
+int bcm63xx_nvram_get_psi_size(void);
+
 #endif /* BCM63XX_NVRAM_H */
