From 8a38220c6bf6d79ecb1c95b083e062bd7221dea9 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Sat, 9 Aug 2025 13:24:57 +0200
Subject: [PATCH] cpufreq: airoha: Add support for AN7583 SoC

New Airoha AN7583 SoC use the same exact logic to control the CPU
frequency. Add the Device compatible to the block list for
cpufreq-dt-plat and to the Airoha CPUFreq driver compatible list.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/cpufreq/airoha-cpufreq.c     | 1 +
 drivers/cpufreq/cpufreq-dt-platdev.c | 1 +
 2 files changed, 2 insertions(+)

--- a/drivers/cpufreq/airoha-cpufreq.c
+++ b/drivers/cpufreq/airoha-cpufreq.c
@@ -121,6 +121,7 @@ static struct platform_driver airoha_cpu
 };
 
 static const struct of_device_id airoha_cpufreq_match_list[] __initconst = {
+	{ .compatible = "airoha,an7583" },
 	{ .compatible = "airoha,en7581" },
 	{},
 };
--- a/drivers/cpufreq/cpufreq-dt-platdev.c
+++ b/drivers/cpufreq/cpufreq-dt-platdev.c
@@ -103,6 +103,7 @@ static const struct of_device_id allowli
  * platforms using "operating-points-v2" property.
  */
 static const struct of_device_id blocklist[] __initconst = {
+	{ .compatible = "airoha,an7583", },
 	{ .compatible = "airoha,en7581", },
 
 	{ .compatible = "allwinner,sun50i-h6", },
