From cb8a4adb586c5e926e415ac0dae3ffb4af30b0a9 Mon Sep 17 00:00:00 2001
From: Andrew Scheller <andrew.scheller@raspberrypi.com>
Date: Thu, 19 Oct 2023 14:13:36 +0100
Subject: [PATCH] Typo in overlays README

touchscreen-size-y for rpi-ft5406 defaults to 480, not 600
---
 arch/arm/boot/dts/overlays/README | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -3738,7 +3738,7 @@ Name:   rpi-ft5406
 Info:   Official Raspberry Pi display touchscreen
 Load:   dtoverlay=rpi-ft5406,<param>=<val>
 Params: touchscreen-size-x      Touchscreen X resolution (default 800)
-        touchscreen-size-y      Touchscreen Y resolution (default 600);
+        touchscreen-size-y      Touchscreen Y resolution (default 480);
         touchscreen-inverted-x  Invert touchscreen X coordinates (default 0);
         touchscreen-inverted-y  Invert touchscreen Y coordinates (default 0);
         touchscreen-swapped-x-y Swap X and Y cordinates (default 0);
