From 546f0617a22a481f3ca1f7e058aea0c40517c64e Mon Sep 17 00:00:00 2001
From: Kathiravan T <quic_kathirav@quicinc.com>
Date: Fri, 26 May 2023 18:23:04 +0530
Subject: [PATCH] arm64: dts: qcom: ipq6018: add QFPROM node

IPQ6018 has efuse region to determine the various HW quirks. Lets
add the initial support and the individual fuses will be added as they
are required.

Signed-off-by: Kathiravan T <quic_kathirav@quicinc.com>
Reviewed-by: Dmitry Baryshkov <dmitry.baryshkov@linaro.org>
Reviewed-by: Konrad Dybcio <konrad.dybcio@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20230526125305.19626-4-quic_kathirav@quicinc.com
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -312,6 +312,13 @@
 			status = "disabled";
 		};
 
+		qfprom: efuse@a4000 {
+			compatible = "qcom,ipq6018-qfprom", "qcom,qfprom";
+			reg = <0x0 0x000a4000 0x0 0x2000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+		};
+
 		prng: qrng@e3000 {
 			compatible = "qcom,prng-ee";
 			reg = <0x0 0x000e3000 0x0 0x1000>;
