From f4f0c8acee0e41c5fbae7a7ad06087668ddce0d6 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Fri, 26 May 2023 21:08:54 +0200
Subject: [PATCH] clk: qcom: gcc-ipq6018: update UBI32 PLL

Update the UBI32 alpha PLL config to the latest values from the downstream
QCA 5.4 kernel.

Signed-off-by: Robert Marko <robimarko@gmail.com>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20230526190855.2941291-1-robimarko@gmail.com
---
 drivers/clk/qcom/gcc-ipq6018.c | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

--- a/drivers/clk/qcom/gcc-ipq6018.c
+++ b/drivers/clk/qcom/gcc-ipq6018.c
@@ -4143,15 +4143,20 @@ static struct clk_branch gcc_dcc_clk = {
 
 static const struct alpha_pll_config ubi32_pll_config = {
 	.l = 0x3e,
-	.alpha = 0x57,
+	.alpha = 0x6667,
 	.config_ctl_val = 0x240d6aa8,
 	.config_ctl_hi_val = 0x3c2,
+	.config_ctl_val = 0x240d4828,
+	.config_ctl_hi_val = 0x6,
 	.main_output_mask = BIT(0),
 	.aux_output_mask = BIT(1),
 	.pre_div_val = 0x0,
 	.pre_div_mask = BIT(12),
 	.post_div_val = 0x0,
 	.post_div_mask = GENMASK(9, 8),
+	.alpha_en_mask = BIT(24),
+	.test_ctl_val = 0x1C0000C0,
+	.test_ctl_hi_val = 0x4000,
 };
 
 static const struct alpha_pll_config nss_crypto_pll_config = {
