From 221581c59c0047b73bc36c12c9c3b42788095823 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Fri, 17 Feb 2023 13:36:36 +0100
Subject: [PATCH] dt-bindings: display: Add BCM2712 MOPLET bindings

The BCM2712 has a MOPLET controller which is basically a TXP without the
transpose feature.

Express that by adding a new compatible for it.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 Documentation/devicetree/bindings/display/brcm,bcm2835-txp.yaml | 1 +
 1 file changed, 1 insertion(+)

--- a/Documentation/devicetree/bindings/display/brcm,bcm2835-txp.yaml
+++ b/Documentation/devicetree/bindings/display/brcm,bcm2835-txp.yaml
@@ -13,6 +13,7 @@ properties:
   compatible:
     enum:
       - brcm,bcm2712-mop
+      - brcm,bcm2712-moplet
       - brcm,bcm2835-txp
 
   reg:
